|  |  |  |
| --- | --- | --- |
| Alloy grades | Types of ingots | Dimensions |
| MA2-1MA2-1pchMA5MA15MA14MA20VMD10 - according to TUMG - according to TU  | Magnesium ingots of round cross-section |  diameter: 370 mm, 460 mm, 530 mm |
| Flat magnesium ingots with cross-section |  165х550 mm, maximum length 5500 mm 190х640 mm, maximum length 5500 mm |