|  |  |  |
| --- | --- | --- |
| Alloy grades | Types of ingots | Dimensions |
| MA2-1  MA2-1pch  MA5  MA15  MA14  MA20  VMD10 - according to TU  MG - according to TU | Magnesium ingots of round cross-section | diameter: 370 mm, 460 mm, 530 mm |
| Flat magnesium ingots with cross-section | 165х550 mm, maximum length 5500 mm    190х640 mm, maximum length 5500 mm |